Micro was a real-time operator and dedicated multi-user.  His broad-band
protocol made it easy for him to interface with numerous input/output devices,
even if it meant time-sharing.

One evening he arrived home just as the Sun was crashing, and had parked his
Motorola 68040 in the main drive (he had missed the 5100 bus that morning),
when he noticed an elegant piece of liveware admiring the daisy wheels in his
garden.  He thought to himself, "She looks user-friendly.  I'll see if she'd
like an update tonight."

Mini was her name, and she was delightfully engineered with eyes like COBOL
and a PR1ME mainframe architecture that set Micro's peripherals networking
all over the place.

He browsed over to her casually, admiring the power of her twin, 32-bit
floating point processors and enquired "How are you, Honeywell?".  "Yes, I am
well", she responded, batting her optical fibers engagingly and smoothing her
console over her curvilinear functions.

Micro settled for a straight line approximation.  "I'm stand-alone tonight",
he said, "How about computing a vector to my base address?  I'll output a
byte to eat, and maybe we could get offset later on."

Mini ran a priority process for 2.6 milliseconds, then transmitted 8 K.  "I've
been dumped myself recently, and a new page is just what I need to refresh my
disks.  I'll park my machine cycle in your background and meet you inside."
She walked off, leaving Micro admiring her solenoids and thinking, "Wow, what
a global variable, I wonder if she'd like my firmware?"

They sat down at the process table to top of form feed of fiche and chips and a
bucket of baudot.  Mini was in conversation mode and expanded on ambiguous
arguments while Micro gave the occassional acknowledgements, although, in
reality, he was analyzing the shortest and least critical path to her entry
point.  He finally settled on the old 'Would you like to_see_my_benchmark
routine', but Mini was again one step ahead.

Suddenly she was up and stripping off her parity bits to reveal the full
functionality of her operating system software.  "Let's get BASIC, you RAM",
she said.  Micro was loaded by this; his hardware was in danger of overflowing
its output buffer, a hang-up that Micro had consulted his analyst about.
"Core", was all he could say, as she prepared to log him off.

Micro soon recovered, however, when Mini went down on the DEC and opened her
divide files to reveal her data set ready.  He accessed his fully packed root
device and was just about to start pushing into her CPU stack, when she
attempted an escape sequence.

"No, no!", she cried, "You're not shielded!"

"Reset, Baby", he replied, "I've been debugged."

"But I haven't got my current loop enabled, and I can't support child
processes", she protested.

"Don't run away", he said, "I'll generate an interrupt."

"No, that's too error prone, and I can't abort because of my design
philosophy."

Micro was locked in by this stage, though, and could not be turned off.  But
Mini soon stopped his thrashing by introducing a coltage spike into his main
supply, whereupon he fell over with a head crash and went to sleep.

"Computers!", she thought, as she recompiled herself.  "All they ever think of
is hex!"


