9-12f Electric Wire
(M/g bdsm reluc)

Written by cc




After years of careful research and development, the manufacturers of the famous "9-12f GrooveStrap" proudly present: 

The 9-12f Electric Wire!

	The 9-12f Electric Wire, like the GrooveStrap, is made of the finest natural and synthetic materials. If properly employed it should provide years of disciplinary use and pleasure. This document will serve as combination warranty, directions for use, and contract. Please read it carefully.

	The 9-12f Electric Wire is designed for use only on a 9 to 12 year old preteen girl in the context of a legal, heterosexual, marital relationship (special application may be made for use on an 8-year-old girl). Naturally, owing to the differences in age-of-consent and marriage laws, this restricts the areas of the world in which it may be properly used. That is why the 9-12f Electric Wire is manufactured in ******, and can be shipped only to *****, *****, and *****. 

	NOTE: Use of the 9-12f Electric Wire in a manner not allowed by this contract will void the warranty and may result in civil and criminal penalties. If credible evidence is received that indicates such usage has occurred, the manufacturer of the Electric Wire will initiate contact with the proper authorities and cooperate fully in any investigation.

	The 9-12f Electric Wire is carefully calibrated for use on a preteen girl. While use of the 9-12f Electric Wire on a teenager is not prohibited by contract, unless it is a young teen with little or no pubic hair, the manufacturer recommends using the "T" model Electric Wire, which utilizes a higher current and a thinner wire, resulting in a more intense punishment. 

       Directions for Use: The 9-12f Electric Wire consists of a rheostat system, two adjustable stands connected by both an adjustable base and a length of wire specially chosen for its gauge and conductive properties, and two switches which will be described further below. It runs on standard house current, and employs a triple-safe system to prevent accidental electrical discharge. 
       
       Set-Up: Position the stands far enough apart to keep the wire at medium tension. The two switches are secured on either side of the base, midway along the wire. The preteen girl should be given a full introduction to the operation of the instrument before being made to stand straddling the wire, with her heels resting with normal weight on each of the switches. When the switches are depressed in this manner, the flow of current through the wire is cut off.

	Now raise the height of each stand until the wire presses firmly into the preteen girl's clitoris, vulva, and anus. When sufficient tension is applied, this should cause the girl to raise up on her toes to relieve the pressure of the wire upon her intimate parts. This allows the current to flow through the wire, which is now so firmly applied to her cleft and anus. If the preteen has been properly instructed, after a few moments of this, she will press her heels back down against the switches so as to cut off the current. If the tension of the wire has been properly adjusted, this should cause the wire to "cut in" to her tenderness sufficiently firmly that she will soon choose to raise up again on her toes, thus coming full circle in her punishment.

	When used on most preteen girls, this should result in a fetching display, as she bounces up and down on the wire, tiptoe to flatfoot and back again. Naturally many operators may choose to supplement the punishment with judicious use of the switch, crop, or belt, on her thighs, bottom, or little breasts, as she bounces up and down(the 9-12f GrooveStrap is, unfortunately, not suited to this function, being designed for use directly on the preteen girl's anus, vulva, and clitoris).

	NOTE: The gauge of the wire and the function of the rheostat have been carefully selected so as to render it very difficult to apply enough pressure or current to damage the skin of a preteen girl. Any attempt, such as tampering with the rheostat or the wire, to thwart this design so as to produce damage, will void the warranty and render the user liable to the penalties described above. 

       Mr ****, a satisfied customer from ****, has graciously allowed us to reprint his letter to us by way of testimony:

	"I recently purchased the 9-12f Electric Wire, and thought I'd describe to you how well it worked. I have a preteen girl, about 10 years old. She is a pretty little thing, very slender and somber, except when she lights up the room with one of her rare smiles. I found her on the streets of **** in **** a few years ago, having been recently abandoned. She was unsure of her own birthday, so we don't know exactly how old she is. Fortunately she had suffered nothing worse than malnutrition. After the appropriate bribes, etc, I succeeded in adopting her despite being a single male. I then moved to **** with her so that, again after sufficient inducements were offered to the applicable officials, I was able to marry her legally, so that I could cherish her, care for her, teach her, and punish her properly. 

	I began her punishment by tossing up her skirt (I do not allow her to wear panties), bending her under my arm, and giving her a brisk, business-like spanking on her bare bottom, accompanied by her usual moans and cries. I then applied a switch to her thighs, back and front, leaving a network of thin red lines that faded slowly. At this point I stripped her, leaving her standing naked in front of me. She is still shy and inhibited, and it always embarrasses her to be only ten years old and have a grown man see her unfledged nakedness. She whimpered, and blushed prettily down to the tips of her little breasts. I continued to whip her with the switch, first on her bottom, then on her little nipples and breastbuds. This left her moaning and sobbing a bit, her nipples erect and fetchingly reddened. I finished her whipping with a few strokes directly on her mons and girlcleft, making her cry out, but I didn't spend as much time punishing her vulva as I usually do, being in a hurry to try out the Electric Wire!

	I had set up the apparatus previously in an adjoining room, and now took her in to see it. Her eyes widened as I explained its function. I pointed out the switches, and let her feel the current briefly with her fingers when the switches were released.

	I turned it off, picked her up and put her down straddling the wire, her heels depressing the switches. I turned the unit back on (the rheostat makes a very noticeable hum; nice touch!). Then I adjusted the stands upward. As the wire pressed firmly onto her unfledged cleft, clitoris, and anus she trembled and moaned.

	Finally she was forced onto her toes, releasing the switches. She cried out as the electricity flowed through the wire (I really like the "zzzzz!" sound the unit produces at this point!), punishing her tender parts. She quickly brought her heels back down onto the switches, but was unable to keep them there long, owing to the pressure of the wire. She went back up on her toes, only to find the current flowing again through her clitoris, cleft, and anus. So she bounced up and down, spending a second or two in each position before being forced, with a cry, to depress or release the switches. Her buttocks jiggled prettily, as did her breasts, at least to the limit that their small size allowed.

	After taking in this pleasing spectacle for a short while, I elected to augment the punishment with a riding crop judiciously applied to her bottom, thighs, and nipples.

	It wasn't long before the stimulation was so intense (both for her and for me!) that I whisked her off the wire and held her close. She clung to me fiercely, shivering and moaning, her tears staining my collar. I then took her to bed, where I finished her punishment with a stern raping, covering her small slender body with mine, thrusting my rod repeatedly into her unfledged preteen girlhood as she cried out and came.

Thank You, 9-12f Electric Wire!

Sincerely, Mr. **********, *****" 

	

by cc
	

All comments gluttonously desired!

ccccc12345@lavabit.com
	

